Arachne Video Setup | Arachne detected video adapter:

CGA 640x200 16 KB 2 shades |

EGA 640x350 128 KB 16 colors

VESA compatible card or driver VGA 640x480 256 KB 16 colors
VGA 640x480 256 KB grayscale
TRIDENT (or PROVGA_VC510S)
TSG3 (Tseng ET3000, MDB10)
OAK
REALTEK (RTVGA)
TSG4 (Tseng ET4000)
M1 (OCTEK, graphic chip MX86010)
TAMARA (Tamarack TDVGA-3588, Cirrus, Paradise, AST-PLUS)
| 640x480 | 1 MB HiColor 800x600 | 1 MB HiColor
1024x768 | 2 MB HiColor
1280x1024 | 4 MB HiColor
1600x1200 | 4 MB HiColor
640x400 | 256 KB 256 colors
640x480 | 512 KB 256 colors
800x600 | 512 KB 256 colors
1024x768 | 1 MB 256 colors
800x600 | 256 KB 16 colors
800x600 | 256 KB grayscale

1) Pick the default setup by clicking on "Try selected graphics mode" (Recommended for beginners)
... alternately....
2a) Pick a card type by tabbing to appropriate check box and pressing enter..or..'leftclick' on appropriate check box.
2b) Pick a size/color resolution in the same manner (tab/enter or leftclick).
2c) Tab/Enter or leftclick on "Try selected graphics mode".